*
*******************************************
*
*BZV55-C47
*
*NXP Semiconductors
*
*Voltage regulator diode
*
*
*
*
* 
*
*IR    = 50nA  @ VR   = 0,7V
*IZSM  = 0,5A  @ tp   = 100µs
*VZmax = 50,0V @ IZ   = 2mA
*VZSM  =       @ IZSM =
*
*
*
* 
*
*
*Package pinning does not match Spice model pinning.
*Package: SOD80C
*
*Package Pin 1: Cathode      
*Package Pin 2: Anode
*
*
*
*
*Simulator: SPICE2
*
*******************************************
*#
.SUBCKT BZV55-C47 1 2
*
*The resistor R1 and the diode D2 do not reflect 
*physical devices but improve 
*only modeling in the reverse 
*mode of operation.
*
R1 1 2 5E+011
D1 1 2 DIODE1
D2 1 2 DIODE2
*
.MODEL DIODE1 D
+ IS = 8E-013
+ N = 1.3
+ BV = 45.97
+ IBV = 3.477E-010
+ RS = 0.3
+ CJO = 1.682E-011
+ VJ = 0.8
+ M = 0.41
+ FC = 0.5
+ TT = 0
+ EG = 1.1
+ XTI = 3
.MODEL DIODE2 D
+ IS = 3E-015
+ N = 1.2
+ RS = 250
.ENDS
*

