*
*******************************************
*
*BZX84-C4V7
*
*NXP Semiconductors
*
*Voltage regulator diode
*
*
*
*
* 
*
*IR    = 3µA @ VR = 2V
*IZSM  = 6A  @ tp = 100µs
*VZmax = 5V  @ IZ = 5mA
*
*
*
*
* 
*
*
*Package pinning does not match Spice model pinning.
*Package: SOT23
*
*Package Pin 1: Anode
*Package Pin 2: not connected
*Package Pin 3: Cathode
*
*
*
*Simulator: SPICE3
*
*******************************************
*#
.SUBCKT BZX84-C4V7 1 2   
 R1 1 2 1E+010   
 D1 1 2  
 + DIODE1
 D2 3 1  
 + DIODE2
 VZ 2 3 0.2      
*
*The resistor R1, the diode D2 and   
*VZ do not  reflect  
*physical devices but improve 
*only modeling in the reverse 
*mode of operation.
*
.MODEL DIODE1 D 
 + IS = 1E-014   
 + N = 1.1       
 + BV = 4.53     
 + IBV = 1E-009  
 + RS = 0.6      
 + CJO = 1.316E-010      
 + VJ = 0.6      
 + M = 0.31      
 + FC = 0.5      
 + TT = 0
 + EG = 1.1      
 + XTI = 3       
 .MODEL DIODE2 D 
 + IS = 8E-011   
 + N = 9.5       
 + RS = 6
 .ENDS 
 *
